Time Control Solution

Implement Timer feature with ROCKEY6 SMART

This sample solution intends to implement Timer function with the support of ROCKEY6 SMART; particularly, it achieved software license control by creating built-in timer program of the dongle, being independent of the system clock.

Before using, it begins with setting the valid time limit (minutes) and creating time information file (in-line file). Note the time can be set one time only, and the original time informtaion file should be deleted if time resetting is required.  

The Timer program will run two times as the software start up, the first is time counting preparation, and at the second time it begins to count time; from now on, you cannot terminate the timing function before quitting the software.  
